**To plan & complete the servicing of below listed plant valve's for better operation & performance 1)Hydrogen caloric PSA valve.2)H2 Linde PSA Valve,3)Nitrogen Plant PSA valve 4)Natural Gas Skid 5)H2 Loop Reactor valve**

100 % Completed as per schedule & clearance’s per Instrument shutdwn Job list clearance maintenance job carried out & it's working satisfactory after maintenance.Also assurance given for the functioning of serviced instruments:1)Hydrogen caloric PSA valve: Hydrogen Caloric Plant PSA valve servicing carried out every 1.5 years for avoiding the downtime/failure.Last time servicing carried out in February'2016.2)H2 Linde PSA Valve: Hydrogen Linde Plant PSA valve servicing carried out every 1.5 years for avoiding the downtime/failure. Last time servicing carried out in May'2016.3)Nitrogen Plant PSA valve :Nitrogen plant PSA valve servicing carried out every 1.0 years for avoiding the downtime/failure. Also al 9 no's Actuator servicing carried out. Last servicing done in November'2016.4)Natural Gas Skid:2 Bar & 4 Bar==Both Skid servicing & overhauling carried out in October'2016.5)H2 Loop Reactor valve:Control valve PCV-302A/PCV-701BV,XV-311,XV-306,XV-306B servicing & overhauling carried out in September & October'2016.Also extra 5 no's valve made ready as a critical spares for Hydroegn PSA & Nitrogen PSA.